Select Network Card Interface

Choose which IP is the Default Internet facing IP Address. (Default gateway)

XXX.XXX.XXX.XXX

External IP Configuration

Static Public IP (IP Address does not change)

Enter your static public IP

XXX.XXX.XXX.XXX

Primary STUN server

stun.3cx.com 3478

Secondary STUN server

stun2.3cx.com 3478

Third STUN server

stun3.3cx.com 3478

Timeout time for STUN response (ms)

3000

Query STUN server every (sec)

1200

Fully Qualified Domain Name

The FQDN is used by 3CX for calls, provisioning URLS and client configuration. It can not be changed afterwards.

<Site>

Settings for Direct SIP Calls

3CX Phone System can make or receive Direct SIP Calls (user1@mydomain.com) as well as place Direct SIP calls to other domains. Requires DNS SRV records. Click here for more info..

Local SIP domain

<Site>

SIP Port

SIP port used by PBX

5060

Tunnel Port

Tunnel Listening port

5090

Settings

Send Media to IP and port of REGISTER