Dell PowerEdge FC630

Xeon Ghz cores each

1 Slim PERC Controller for Raid

1 Qlogic RNA Blade Network daughter card. For Fibre Channel

RDimm 2400 MT/s. 256 Gb Total

SSD 6 Gb/s

Optional and recommended Add-ons

-Samsung Autocache. To be use with VMware Vsphere 6.01u+

-Dell EMC PE Express Flash NVME (SSD). It provides LB and FO

-Fail-Safer Hypervisor using SD Cards in Raid 1. Installing the Hypervisor on a SD card